You need to import categories of transport in your system.

**Table of categories of transport in the rights of technical categories**

| **Category** | **Technical category of vehicle** |
| --- | --- |
| M | L1 (excluding bicycles), L6 |
| A | L3 |
| A1 | L3 на <= 125 см3 и макс. мощностью <= 11 киловатт (но не L1) |
| B | M1/N1, whose maximum weight does not exceed 3.5 tons; M1/N1+O1; M1/N1 |
| BE | M1, whose permissible maximum weight does not exceed 3.5 tons, with a trailer heavier than it (above 3.5 tons together) |
| B1 | L2, L4, L5, L7 |
| С | M1/N2/N3, whose maximum weight exceeds 3.5 tons (but not M2 / M3) |
| С1 | M1/N2, the permitted maximum weight of which is 3.5-7.5 tons (but not M2 / M3), is possible with O1 |
| С1E | M1/N2, the maximum weight of which is 3.5-7.5 tons (but not M2 / M3), with a trailer> 750kg (up to 12 tons together) |
| СE | M1/N2/N3, whose permissible maximum mass exceeds 3.5 tons (but not M2 / M3) coupled to a trailer> 750kg |
| D | M2/M3, possible with O1 |
| D1 | M2/M3 no more than with 16 passenger seats, it is possible with O1 |
| D1E | M2/M3 no more than with 16 passenger seats and with an O1 not intended for passengers (up to 12 tons together) |
| DE | M2/M3 with trailer> 750 kg; articulated buses, duobus. |
| Tm | M2/M3, being trams |
| Tb | M2/M3, rolleybuses |